// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "tplink,eap245-v3", "qca,qca9563";
	model = "TP-Link EAP245 v3 / EAP265 HD v1";

	aliases {
		led-boot = &led_status_green;
		led-failsafe = &led_status_amber;
		led-running = &led_status_green;
		led-upgrade = &led_status_amber;
		label-mac-device = &eth0;
	};

	leds {
		compatible = "gpio-leds";

		led_status_green: status_green {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		led_status_amber: status_amber {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpio 9 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0 0 0 0 0>;

		nvmem-cells = <&macaddr_info_8 1>, <&calibration_ath10k>;
		nvmem-cell-names = "mac-address", "pre-calibration";
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "factory-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot";
				reg = <0x040000 0x040000>;
				read-only;
			};

			partition@80000 {
				label = "partition-table";
				reg = <0x080000 0x010000>;
				read-only;
			};

			info: partition@90000 {
				label = "info";
				reg = <0x090000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_info_8: macaddr@8 {
						compatible = "mac-base";
						reg = <0x8 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@a0000 {
				label = "art";
				reg = <0x0a0000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					calibration_ath9k: calibration@1000 {
						reg = <0x1000 0x440>;
					};

					calibration_ath10k: calibration@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};

			partition@b0000 {
				label = "extra-para";
				reg = <0x0b0000 0x010000>;
				read-only;
			};

			partition@c0000 {
				compatible = "openwrt,elf";
				label = "firmware";
				reg = <0x0c0000 0xe40000>;
			};

			partition@f00000 {
				label = "config";
				reg = <0xf00000 0x030000>;
				read-only;
			};

			partition@f30000 {
				label = "mutil-log";
				reg = <0xf30000 0x080000>;
				read-only;
			};

			partition@fb0000 {
				label = "oops";
				reg = <0xfb0000 0x040000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";
		qca,ar8327-initvals = <
			0x04 0x00080080 /* PAD0 */
			0x7c 0x0000007e /* PORT0_STATUS */
			0xe0 0xc74164de /* SGMII_CTRL */
			>;
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy0>;
	phy-mode = "sgmii";

	nvmem-cells = <&macaddr_info_8 0>;
	nvmem-cell-names = "mac-address";
};

&wmac {
	status = "okay";

	nvmem-cells = <&macaddr_info_8 0>, <&calibration_ath9k>;
	nvmem-cell-names = "mac-address", "calibration";
};
