From 2b88563ee5aafd9571d965b7f2093a0f58d98a31 Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Thu, 26 Nov 2020 12:02:21 +0100
Subject: net: dsa: Increase max ports for rtl838x

* rename the target to realtek
* add refactored DSA driver
* add latest gpio driver
* lots of arch cleanups
* new irq driver
* additional boards

Submitted-by: Bert Vermeulen <bert@biot.com>
Submitted-by: Birger Koblitz <mail@birger-koblitz.de>
Submitted-by: Sander Vanheule <sander@svanheule.net>
Submitted-by: Bjørn Mork <bjorn@mork.no>
Submitted-by: John Crispin <john@phrozen.org>
---
 include/linux/platform_data/dsa.h             | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/include/linux/platform_data/dsa.h
+++ b/include/linux/platform_data/dsa.h
@@ -6,7 +6,7 @@ struct device;
 struct net_device;
 
 #define DSA_MAX_SWITCHES	4
-#define DSA_MAX_PORTS		12
+#define DSA_MAX_PORTS		54
 #define DSA_RTABLE_NONE		-1
 
 struct dsa_chip_data {
