// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca953x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	compatible = "kuwfi,c910", "qca,qca9533";
	model = "KuWFi C910";

	aliases {
		label-mac-device = &eth1;
		led-boot = &internet_red;
		led-failsafe = &internet_red;
		led-upgrade = &internet_red;
	};

	virtual_flash {
		compatible = "mtd-concat";
		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x0>;
				label = "firmware";
				compatible = "openwrt,uimage", "denx,uimage";
				openwrt,ih-magic = <IH_MAGIC_OKLI>;
			};
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		internet_blue {
			label = "blue:internet";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		wifi {
			label = "white:wifi";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		internet_green {
			label = "green:internet";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		wan {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		lan2 {
			label = "white:lan2";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};

		// gpio 12 enables or disables LTE (Quectel EC200T)

		internet_red: internet_red {
			label = "red:internet";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		lan1 {
			label = "white:lan1";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "winbond,w25q128", "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				label = "u-boot-env";
				reg = <0x020000 0x010000>;
				read-only;
			};

			partition@30000 {
				label = "config";
				reg = <0x030000 0x020000>;
				read-only;
			};

			fwconcat0: partition@50000 {
				label = "fwconcat0";
				reg = <0x050000 0xe30000>;
			};

			partition@e80000 {
				label = "loader";
				reg = <0xe80000 0x10000>;
			};

			fwconcat1: partition@e90000 {
				label = "fwconcat1";
				reg = <0xe90000 0x160000>;
			};

			partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					calibration_art_1000: macaddr@1000 {
						reg = <0x1000 0x440>;
					};

					macaddr_art_1002: macaddr@1002 {
						compatible = "mac-base";
						reg = <0x1002 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};
		};
	};
};

&usb0 {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&eth0 {
	status = "okay";

	phy-handle = <&swphy0>;

	nvmem-cells = <&macaddr_art_1002 1>;
	nvmem-cell-names = "mac-address";
};

&eth1 {
	phy-handle = <&swphy4>;

	nvmem-cells = <&macaddr_art_1002 0>;
	nvmem-cell-names = "mac-address";

	gmac-config {
		device = <&gmac>;
		switch-phy-swap = <1>;
	};
};

&wmac {
	status = "okay";

	nvmem-cells = <&calibration_art_1000>;
	nvmem-cell-names = "calibration";
};
