From 0b17197055b528da22e9385200e61b847b499d48 Mon Sep 17 00:00:00 2001
From: Mantas Pucka <mantas@8devices.com>
Date: Thu, 25 Jan 2024 11:04:11 +0200
Subject: [PATCH] arm64: dts: qcom: ipq6018: add tsens node

IPQ6018 has temperature sensing HW block compatible with IPQ8074. Add
node for it.

Signed-off-by: Mantas Pucka <mantas@8devices.com>
Link: https://lore.kernel.org/r/1706173452-1017-3-git-send-email-mantas@8devices.com
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
---
 arch/arm64/boot/dts/qcom/ipq6018.dtsi | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/arch/arm64/boot/dts/qcom/ipq6018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq6018.dtsi
@@ -343,6 +343,16 @@
 			clock-names = "core";
 		};
 
+		tsens: thermal-sensor@4a9000 {
+			compatible = "qcom,ipq6018-tsens", "qcom,ipq8074-tsens";
+			reg = <0x0 0x004a9000 0x0 0x1000>,
+			      <0x0 0x004a8000 0x0 0x1000>;
+			interrupts = <GIC_SPI 184 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "combined";
+			#qcom,sensors = <16>;
+			#thermal-sensor-cells = <1>;
+		};
+
 		cryptobam: dma-controller@704000 {
 			compatible = "qcom,bam-v1.7.0";
 			reg = <0x0 0x00704000 0x0 0x20000>;
