From d788961c5b25d9d822c4230bfbc536a6736b91ff Mon Sep 17 00:00:00 2001
From: Gatien Chevallier <gatien.chevallier@foss.st.com>
Date: Fri, 5 Jan 2024 14:04:03 +0100
Subject: [PATCH 1/5] ARM: dts: stm32: add ETZPC as a system bus for STM32MP13x
 boards

ETZPC is a firewall controller. Put all peripherals filtered by the
ETZPC as ETZPC subnodes and keep the "simple-bus" compatible for
backward compatibility.

Signed-off-by: Gatien Chevallier <gatien.chevallier@foss.st.com>
Signed-off-by: Alexandre Torgue <alexandre.torgue@foss.st.com>
---
 arch/arm/boot/dts/st/stm32mp131.dtsi  | 1020 +++++++++++++------------
 arch/arm/boot/dts/st/stm32mp133.dtsi  |   50 +-
 arch/arm/boot/dts/st/stm32mp13xc.dtsi |   18 +-
 arch/arm/boot/dts/st/stm32mp13xf.dtsi |   18 +-
 4 files changed, 569 insertions(+), 537 deletions(-)

--- a/arch/arm/boot/dts/st/stm32mp131.dtsi
+++ b/arch/arm/boot/dts/st/stm32mp131.dtsi
@@ -745,340 +745,6 @@
 			dma-channels = <16>;
 		};
 
-		adc_2: adc@48004000 {
-			compatible = "st,stm32mp13-adc-core";
-			reg = <0x48004000 0x400>;
-			interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc ADC2>, <&rcc ADC2_K>;
-			clock-names = "bus", "adc";
-			interrupt-controller;
-			#interrupt-cells = <1>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			status = "disabled";
-
-			adc2: adc@0 {
-				compatible = "st,stm32mp13-adc";
-				#io-channel-cells = <1>;
-				#address-cells = <1>;
-				#size-cells = <0>;
-				reg = <0x0>;
-				interrupt-parent = <&adc_2>;
-				interrupts = <0>;
-				dmas = <&dmamux1 10 0x400 0x80000001>;
-				dma-names = "rx";
-				status = "disabled";
-
-				channel@13 {
-					reg = <13>;
-					label = "vrefint";
-				};
-				channel@14 {
-					reg = <14>;
-					label = "vddcore";
-				};
-				channel@16 {
-					reg = <16>;
-					label = "vddcpu";
-				};
-				channel@17 {
-					reg = <17>;
-					label = "vddq_ddr";
-				};
-			};
-		};
-
-		usbotg_hs: usb@49000000 {
-			compatible = "st,stm32mp15-hsotg", "snps,dwc2";
-			reg = <0x49000000 0x40000>;
-			clocks = <&rcc USBO_K>;
-			clock-names = "otg";
-			resets = <&rcc USBO_R>;
-			reset-names = "dwc2";
-			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
-			g-rx-fifo-size = <512>;
-			g-np-tx-fifo-size = <32>;
-			g-tx-fifo-size = <256 16 16 16 16 16 16 16>;
-			dr_mode = "otg";
-			otg-rev = <0x200>;
-			usb33d-supply = <&scmi_usb33>;
-			status = "disabled";
-		};
-
-		usart1: serial@4c000000 {
-			compatible = "st,stm32h7-uart";
-			reg = <0x4c000000 0x400>;
-			interrupts-extended = <&exti 26 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc USART1_K>;
-			resets = <&rcc USART1_R>;
-			wakeup-source;
-			dmas = <&dmamux1 41 0x400 0x5>,
-			       <&dmamux1 42 0x400 0x1>;
-			dma-names = "rx", "tx";
-			status = "disabled";
-		};
-
-		usart2: serial@4c001000 {
-			compatible = "st,stm32h7-uart";
-			reg = <0x4c001000 0x400>;
-			interrupts-extended = <&exti 27 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc USART2_K>;
-			resets = <&rcc USART2_R>;
-			wakeup-source;
-			dmas = <&dmamux1 43 0x400 0x5>,
-			       <&dmamux1 44 0x400 0x1>;
-			dma-names = "rx", "tx";
-			status = "disabled";
-		};
-
-		i2s4: audio-controller@4c002000 {
-			compatible = "st,stm32h7-i2s";
-			reg = <0x4c002000 0x400>;
-			#sound-dai-cells = <0>;
-			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
-			dmas = <&dmamux1 83 0x400 0x01>,
-			       <&dmamux1 84 0x400 0x01>;
-			dma-names = "rx", "tx";
-			status = "disabled";
-		};
-
-		spi4: spi@4c002000 {
-			compatible = "st,stm32h7-spi";
-			reg = <0x4c002000 0x400>;
-			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc SPI4_K>;
-			resets = <&rcc SPI4_R>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			dmas = <&dmamux1 83 0x400 0x01>,
-			       <&dmamux1 84 0x400 0x01>;
-			dma-names = "rx", "tx";
-			status = "disabled";
-		};
-
-		spi5: spi@4c003000 {
-			compatible = "st,stm32h7-spi";
-			reg = <0x4c003000 0x400>;
-			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc SPI5_K>;
-			resets = <&rcc SPI5_R>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			dmas = <&dmamux1 85 0x400 0x01>,
-			       <&dmamux1 86 0x400 0x01>;
-			dma-names = "rx", "tx";
-			status = "disabled";
-		};
-
-		i2c3: i2c@4c004000 {
-			compatible = "st,stm32mp13-i2c";
-			reg = <0x4c004000 0x400>;
-			interrupt-names = "event", "error";
-			interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>,
-				     <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc I2C3_K>;
-			resets = <&rcc I2C3_R>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			dmas = <&dmamux1 73 0x400 0x1>,
-			       <&dmamux1 74 0x400 0x1>;
-			dma-names = "rx", "tx";
-			st,syscfg-fmp = <&syscfg 0x4 0x4>;
-			i2c-analog-filter;
-			status = "disabled";
-		};
-
-		i2c4: i2c@4c005000 {
-			compatible = "st,stm32mp13-i2c";
-			reg = <0x4c005000 0x400>;
-			interrupt-names = "event", "error";
-			interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>,
-				     <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc I2C4_K>;
-			resets = <&rcc I2C4_R>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			dmas = <&dmamux1 75 0x400 0x1>,
-			       <&dmamux1 76 0x400 0x1>;
-			dma-names = "rx", "tx";
-			st,syscfg-fmp = <&syscfg 0x4 0x8>;
-			i2c-analog-filter;
-			status = "disabled";
-		};
-
-		i2c5: i2c@4c006000 {
-			compatible = "st,stm32mp13-i2c";
-			reg = <0x4c006000 0x400>;
-			interrupt-names = "event", "error";
-			interrupts = <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>,
-				     <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc I2C5_K>;
-			resets = <&rcc I2C5_R>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			dmas = <&dmamux1 115 0x400 0x1>,
-			       <&dmamux1 116 0x400 0x1>;
-			dma-names = "rx", "tx";
-			st,syscfg-fmp = <&syscfg 0x4 0x10>;
-			i2c-analog-filter;
-			status = "disabled";
-		};
-
-		timers12: timer@4c007000 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			compatible = "st,stm32-timers";
-			reg = <0x4c007000 0x400>;
-			interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
-			interrupt-names = "global";
-			clocks = <&rcc TIM12_K>;
-			clock-names = "int";
-			status = "disabled";
-
-			pwm {
-				compatible = "st,stm32-pwm";
-				#pwm-cells = <3>;
-				status = "disabled";
-			};
-
-			timer@11 {
-				compatible = "st,stm32h7-timer-trigger";
-				reg = <11>;
-				status = "disabled";
-			};
-		};
-
-		timers13: timer@4c008000 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			compatible = "st,stm32-timers";
-			reg = <0x4c008000 0x400>;
-			interrupts = <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>;
-			interrupt-names = "global";
-			clocks = <&rcc TIM13_K>;
-			clock-names = "int";
-			status = "disabled";
-
-			pwm {
-				compatible = "st,stm32-pwm";
-				#pwm-cells = <3>;
-				status = "disabled";
-			};
-
-			timer@12 {
-				compatible = "st,stm32h7-timer-trigger";
-				reg = <12>;
-				status = "disabled";
-			};
-		};
-
-		timers14: timer@4c009000 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			compatible = "st,stm32-timers";
-			reg = <0x4c009000 0x400>;
-			interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
-			interrupt-names = "global";
-			clocks = <&rcc TIM14_K>;
-			clock-names = "int";
-			status = "disabled";
-
-			pwm {
-				compatible = "st,stm32-pwm";
-				#pwm-cells = <3>;
-				status = "disabled";
-			};
-
-			timer@13 {
-				compatible = "st,stm32h7-timer-trigger";
-				reg = <13>;
-				status = "disabled";
-			};
-		};
-
-		timers15: timer@4c00a000 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			compatible = "st,stm32-timers";
-			reg = <0x4c00a000 0x400>;
-			interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
-			interrupt-names = "global";
-			clocks = <&rcc TIM15_K>;
-			clock-names = "int";
-			dmas = <&dmamux1 105 0x400 0x1>,
-			       <&dmamux1 106 0x400 0x1>,
-			       <&dmamux1 107 0x400 0x1>,
-			       <&dmamux1 108 0x400 0x1>;
-			dma-names = "ch1", "up", "trig", "com";
-			status = "disabled";
-
-			pwm {
-				compatible = "st,stm32-pwm";
-				#pwm-cells = <3>;
-				status = "disabled";
-			};
-
-			timer@14 {
-				compatible = "st,stm32h7-timer-trigger";
-				reg = <14>;
-				status = "disabled";
-			};
-		};
-
-		timers16: timer@4c00b000 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			compatible = "st,stm32-timers";
-			reg = <0x4c00b000 0x400>;
-			interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
-			interrupt-names = "global";
-			clocks = <&rcc TIM16_K>;
-			clock-names = "int";
-			dmas = <&dmamux1 109 0x400 0x1>,
-			       <&dmamux1 110 0x400 0x1>;
-			dma-names = "ch1", "up";
-			status = "disabled";
-
-			pwm {
-				compatible = "st,stm32-pwm";
-				#pwm-cells = <3>;
-				status = "disabled";
-			};
-
-			timer@15 {
-				compatible = "st,stm32h7-timer-trigger";
-				reg = <15>;
-				status = "disabled";
-			};
-		};
-
-		timers17: timer@4c00c000 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			compatible = "st,stm32-timers";
-			reg = <0x4c00c000 0x400>;
-			interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
-			interrupt-names = "global";
-			clocks = <&rcc TIM17_K>;
-			clock-names = "int";
-			dmas = <&dmamux1 111 0x400 0x1>,
-			       <&dmamux1 112 0x400 0x1>;
-			dma-names = "ch1", "up";
-			status = "disabled";
-
-			pwm {
-				compatible = "st,stm32-pwm";
-				#pwm-cells = <3>;
-				status = "disabled";
-			};
-
-			timer@16 {
-				compatible = "st,stm32h7-timer-trigger";
-				reg = <16>;
-				status = "disabled";
-			};
-		};
-
 		rcc: rcc@50000000 {
 			compatible = "st,stm32mp13-rcc", "syscon";
 			reg = <0x50000000 0x1000>;
@@ -1105,69 +771,6 @@
 			clocks = <&rcc SYSCFG>;
 		};
 
-		lptimer2: timer@50021000 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			compatible = "st,stm32-lptimer";
-			reg = <0x50021000 0x400>;
-			interrupts-extended = <&exti 48 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc LPTIM2_K>;
-			clock-names = "mux";
-			wakeup-source;
-			status = "disabled";
-
-			pwm {
-				compatible = "st,stm32-pwm-lp";
-				#pwm-cells = <3>;
-				status = "disabled";
-			};
-
-			trigger@1 {
-				compatible = "st,stm32-lptimer-trigger";
-				reg = <1>;
-				status = "disabled";
-			};
-
-			counter {
-				compatible = "st,stm32-lptimer-counter";
-				status = "disabled";
-			};
-
-			timer {
-				compatible = "st,stm32-lptimer-timer";
-				status = "disabled";
-			};
-		};
-
-		lptimer3: timer@50022000 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			compatible = "st,stm32-lptimer";
-			reg = <0x50022000 0x400>;
-			interrupts-extended = <&exti 50 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc LPTIM3_K>;
-			clock-names = "mux";
-			wakeup-source;
-			status = "disabled";
-
-			pwm {
-				compatible = "st,stm32-pwm-lp";
-				#pwm-cells = <3>;
-				status = "disabled";
-			};
-
-			trigger@2 {
-				compatible = "st,stm32-lptimer-trigger";
-				reg = <2>;
-				status = "disabled";
-			};
-
-			timer {
-				compatible = "st,stm32-lptimer-timer";
-				status = "disabled";
-			};
-		};
-
 		lptimer4: timer@50023000 {
 			compatible = "st,stm32-lptimer";
 			reg = <0x50023000 0x400>;
@@ -1220,79 +823,10 @@
 			dma-requests = <48>;
 		};
 
-		fmc: memory-controller@58002000 {
-			compatible = "st,stm32mp1-fmc2-ebi";
-			reg = <0x58002000 0x1000>;
-			ranges = <0 0 0x60000000 0x04000000>, /* EBI CS 1 */
-				 <1 0 0x64000000 0x04000000>, /* EBI CS 2 */
-				 <2 0 0x68000000 0x04000000>, /* EBI CS 3 */
-				 <3 0 0x6c000000 0x04000000>, /* EBI CS 4 */
-				 <4 0 0x80000000 0x10000000>; /* NAND */
-			#address-cells = <2>;
-			#size-cells = <1>;
-			clocks = <&rcc FMC_K>;
-			resets = <&rcc FMC_R>;
-			status = "disabled";
-
-			nand-controller@4,0 {
-				compatible = "st,stm32mp1-fmc2-nfc";
-				reg = <4 0x00000000 0x1000>,
-				      <4 0x08010000 0x1000>,
-				      <4 0x08020000 0x1000>,
-				      <4 0x01000000 0x1000>,
-				      <4 0x09010000 0x1000>,
-				      <4 0x09020000 0x1000>;
-				#address-cells = <1>;
-				#size-cells = <0>;
-				interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
-				dmas = <&mdma 24 0x2 0x12000a02 0x0 0x0>,
-				       <&mdma 24 0x2 0x12000a08 0x0 0x0>,
-				       <&mdma 25 0x2 0x12000a0a 0x0 0x0>;
-				dma-names = "tx", "rx", "ecc";
-				status = "disabled";
-			};
-		};
-
-		qspi: spi@58003000 {
-			compatible = "st,stm32f469-qspi";
-			reg = <0x58003000 0x1000>, <0x70000000 0x10000000>;
-			reg-names = "qspi", "qspi_mm";
-			#address-cells = <1>;
-			#size-cells = <0>;
-			interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
-			dmas = <&mdma 26 0x2 0x10100002 0x0 0x0>,
-			       <&mdma 26 0x2 0x10100008 0x0 0x0>;
-			dma-names = "tx", "rx";
-			clocks = <&rcc QSPI_K>;
-			resets = <&rcc QSPI_R>;
-			status = "disabled";
-		};
-
-		sdmmc1: mmc@58005000 {
-			compatible = "st,stm32-sdmmc2", "arm,pl18x", "arm,primecell";
-			arm,primecell-periphid = <0x20253180>;
-			reg = <0x58005000 0x1000>, <0x58006000 0x1000>;
-			interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc SDMMC1_K>;
-			clock-names = "apb_pclk";
-			resets = <&rcc SDMMC1_R>;
-			cap-sd-highspeed;
-			cap-mmc-highspeed;
-			max-frequency = <130000000>;
-			status = "disabled";
-		};
-
-		sdmmc2: mmc@58007000 {
-			compatible = "st,stm32-sdmmc2", "arm,pl18x", "arm,primecell";
-			arm,primecell-periphid = <0x20253180>;
-			reg = <0x58007000 0x1000>, <0x58008000 0x1000>;
-			interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc SDMMC2_K>;
-			clock-names = "apb_pclk";
-			resets = <&rcc SDMMC2_R>;
-			cap-sd-highspeed;
-			cap-mmc-highspeed;
-			max-frequency = <130000000>;
+		crc1: crc@58009000 {
+			compatible = "st,stm32f7-crc";
+			reg = <0x58009000 0x400>;
+			clocks = <&rcc CRC1>;
 			status = "disabled";
 		};
 
@@ -1323,29 +857,6 @@
 			status = "disabled";
 		};
 
-		usbphyc: usbphyc@5a006000 {
-			#address-cells = <1>;
-			#size-cells = <0>;
-			#clock-cells = <0>;
-			compatible = "st,stm32mp1-usbphyc";
-			reg = <0x5a006000 0x1000>;
-			clocks = <&rcc USBPHY_K>;
-			resets = <&rcc USBPHY_R>;
-			vdda1v1-supply = <&scmi_reg11>;
-			vdda1v8-supply = <&scmi_reg18>;
-			status = "disabled";
-
-			usbphyc_port0: usb-phy@0 {
-				#phy-cells = <0>;
-				reg = <0>;
-			};
-
-			usbphyc_port1: usb-phy@1 {
-				#phy-cells = <1>;
-				reg = <1>;
-			};
-		};
-
 		rtc: rtc@5c004000 {
 			compatible = "st,stm32mp1-rtc";
 			reg = <0x5c004000 0x400>;
@@ -1374,6 +885,529 @@
 			};
 		};
 
+		etzpc: bus@5c007000 {
+			compatible = "simple-bus";
+			reg = <0x5c007000 0x400>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges;
+
+			adc_2: adc@48004000 {
+				compatible = "st,stm32mp13-adc-core";
+				reg = <0x48004000 0x400>;
+				interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc ADC2>, <&rcc ADC2_K>;
+				clock-names = "bus", "adc";
+				interrupt-controller;
+				#interrupt-cells = <1>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+				status = "disabled";
+
+				adc2: adc@0 {
+					compatible = "st,stm32mp13-adc";
+					#io-channel-cells = <1>;
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0x0>;
+					interrupt-parent = <&adc_2>;
+					interrupts = <0>;
+					dmas = <&dmamux1 10 0x400 0x80000001>;
+					dma-names = "rx";
+					status = "disabled";
+
+					channel@13 {
+						reg = <13>;
+						label = "vrefint";
+					};
+					channel@14 {
+						reg = <14>;
+						label = "vddcore";
+					};
+					channel@16 {
+						reg = <16>;
+						label = "vddcpu";
+					};
+					channel@17 {
+						reg = <17>;
+						label = "vddq_ddr";
+					};
+				};
+			};
+
+			usbotg_hs: usb@49000000 {
+				compatible = "st,stm32mp15-hsotg", "snps,dwc2";
+				reg = <0x49000000 0x40000>;
+				clocks = <&rcc USBO_K>;
+				clock-names = "otg";
+				resets = <&rcc USBO_R>;
+				reset-names = "dwc2";
+				interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
+				g-rx-fifo-size = <512>;
+				g-np-tx-fifo-size = <32>;
+				g-tx-fifo-size = <256 16 16 16 16 16 16 16>;
+				dr_mode = "otg";
+				otg-rev = <0x200>;
+				usb33d-supply = <&scmi_usb33>;
+				status = "disabled";
+			};
+
+			usart1: serial@4c000000 {
+				compatible = "st,stm32h7-uart";
+				reg = <0x4c000000 0x400>;
+				interrupts-extended = <&exti 26 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc USART1_K>;
+				resets = <&rcc USART1_R>;
+				wakeup-source;
+				dmas = <&dmamux1 41 0x400 0x5>,
+				<&dmamux1 42 0x400 0x1>;
+				dma-names = "rx", "tx";
+				status = "disabled";
+			};
+
+			usart2: serial@4c001000 {
+				compatible = "st,stm32h7-uart";
+				reg = <0x4c001000 0x400>;
+				interrupts-extended = <&exti 27 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc USART2_K>;
+				resets = <&rcc USART2_R>;
+				wakeup-source;
+				dmas = <&dmamux1 43 0x400 0x5>,
+				<&dmamux1 44 0x400 0x1>;
+				dma-names = "rx", "tx";
+				status = "disabled";
+			};
+
+			i2s4: audio-controller@4c002000 {
+				compatible = "st,stm32h7-i2s";
+				reg = <0x4c002000 0x400>;
+				#sound-dai-cells = <0>;
+				interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
+				dmas = <&dmamux1 83 0x400 0x01>,
+				<&dmamux1 84 0x400 0x01>;
+				dma-names = "rx", "tx";
+				status = "disabled";
+			};
+
+			spi4: spi@4c002000 {
+				compatible = "st,stm32h7-spi";
+				reg = <0x4c002000 0x400>;
+				interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc SPI4_K>;
+				resets = <&rcc SPI4_R>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+				dmas = <&dmamux1 83 0x400 0x01>,
+				       <&dmamux1 84 0x400 0x01>;
+				dma-names = "rx", "tx";
+				status = "disabled";
+			};
+
+			spi5: spi@4c003000 {
+				compatible = "st,stm32h7-spi";
+				reg = <0x4c003000 0x400>;
+				interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc SPI5_K>;
+				resets = <&rcc SPI5_R>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+				dmas = <&dmamux1 85 0x400 0x01>,
+				       <&dmamux1 86 0x400 0x01>;
+				dma-names = "rx", "tx";
+				status = "disabled";
+			};
+
+			i2c3: i2c@4c004000 {
+				compatible = "st,stm32mp13-i2c";
+				reg = <0x4c004000 0x400>;
+				interrupt-names = "event", "error";
+				interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>,
+					     <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc I2C3_K>;
+				resets = <&rcc I2C3_R>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+				dmas = <&dmamux1 73 0x400 0x1>,
+				       <&dmamux1 74 0x400 0x1>;
+				dma-names = "rx", "tx";
+				st,syscfg-fmp = <&syscfg 0x4 0x4>;
+				i2c-analog-filter;
+				status = "disabled";
+			};
+
+			i2c4: i2c@4c005000 {
+				compatible = "st,stm32mp13-i2c";
+				reg = <0x4c005000 0x400>;
+				interrupt-names = "event", "error";
+				interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>,
+					     <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc I2C4_K>;
+				resets = <&rcc I2C4_R>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+				dmas = <&dmamux1 75 0x400 0x1>,
+				       <&dmamux1 76 0x400 0x1>;
+				dma-names = "rx", "tx";
+				st,syscfg-fmp = <&syscfg 0x4 0x8>;
+				i2c-analog-filter;
+				status = "disabled";
+			};
+
+			i2c5: i2c@4c006000 {
+				compatible = "st,stm32mp13-i2c";
+				reg = <0x4c006000 0x400>;
+				interrupt-names = "event", "error";
+				interrupts = <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>,
+					     <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc I2C5_K>;
+				resets = <&rcc I2C5_R>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+				dmas = <&dmamux1 115 0x400 0x1>,
+				       <&dmamux1 116 0x400 0x1>;
+				dma-names = "rx", "tx";
+				st,syscfg-fmp = <&syscfg 0x4 0x10>;
+				i2c-analog-filter;
+				status = "disabled";
+			};
+
+			timers12: timer@4c007000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "st,stm32-timers";
+				reg = <0x4c007000 0x400>;
+				interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "global";
+				clocks = <&rcc TIM12_K>;
+				clock-names = "int";
+				status = "disabled";
+
+				pwm {
+					compatible = "st,stm32-pwm";
+					#pwm-cells = <3>;
+					status = "disabled";
+				};
+
+				timer@11 {
+					compatible = "st,stm32h7-timer-trigger";
+					reg = <11>;
+					status = "disabled";
+				};
+			};
+
+			timers13: timer@4c008000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "st,stm32-timers";
+				reg = <0x4c008000 0x400>;
+				interrupts = <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "global";
+				clocks = <&rcc TIM13_K>;
+				clock-names = "int";
+				status = "disabled";
+
+				pwm {
+					compatible = "st,stm32-pwm";
+					#pwm-cells = <3>;
+					status = "disabled";
+				};
+
+				timer@12 {
+					compatible = "st,stm32h7-timer-trigger";
+					reg = <12>;
+					status = "disabled";
+				};
+			};
+
+			timers14: timer@4c009000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "st,stm32-timers";
+				reg = <0x4c009000 0x400>;
+				interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "global";
+				clocks = <&rcc TIM14_K>;
+				clock-names = "int";
+				status = "disabled";
+
+				pwm {
+					compatible = "st,stm32-pwm";
+					#pwm-cells = <3>;
+					status = "disabled";
+				};
+
+				timer@13 {
+					compatible = "st,stm32h7-timer-trigger";
+					reg = <13>;
+					status = "disabled";
+				};
+			};
+
+			timers15: timer@4c00a000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "st,stm32-timers";
+				reg = <0x4c00a000 0x400>;
+				interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "global";
+				clocks = <&rcc TIM15_K>;
+				clock-names = "int";
+				dmas = <&dmamux1 105 0x400 0x1>,
+				<&dmamux1 106 0x400 0x1>,
+				<&dmamux1 107 0x400 0x1>,
+				<&dmamux1 108 0x400 0x1>;
+				dma-names = "ch1", "up", "trig", "com";
+				status = "disabled";
+
+				pwm {
+					compatible = "st,stm32-pwm";
+					#pwm-cells = <3>;
+					status = "disabled";
+				};
+
+				timer@14 {
+					compatible = "st,stm32h7-timer-trigger";
+					reg = <14>;
+					status = "disabled";
+				};
+			};
+
+			timers16: timer@4c00b000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "st,stm32-timers";
+				reg = <0x4c00b000 0x400>;
+				interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "global";
+				clocks = <&rcc TIM16_K>;
+				clock-names = "int";
+				dmas = <&dmamux1 109 0x400 0x1>,
+				<&dmamux1 110 0x400 0x1>;
+				dma-names = "ch1", "up";
+				status = "disabled";
+
+				pwm {
+					compatible = "st,stm32-pwm";
+					#pwm-cells = <3>;
+					status = "disabled";
+				};
+
+				timer@15 {
+					compatible = "st,stm32h7-timer-trigger";
+					reg = <15>;
+					status = "disabled";
+				};
+			};
+
+			timers17: timer@4c00c000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "st,stm32-timers";
+				reg = <0x4c00c000 0x400>;
+				interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "global";
+				clocks = <&rcc TIM17_K>;
+				clock-names = "int";
+				dmas = <&dmamux1 111 0x400 0x1>,
+				       <&dmamux1 112 0x400 0x1>;
+				dma-names = "ch1", "up";
+				status = "disabled";
+
+				pwm {
+					compatible = "st,stm32-pwm";
+					#pwm-cells = <3>;
+					status = "disabled";
+				};
+
+				timer@16 {
+					compatible = "st,stm32h7-timer-trigger";
+					reg = <16>;
+					status = "disabled";
+				};
+			};
+
+			lptimer2: timer@50021000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "st,stm32-lptimer";
+				reg = <0x50021000 0x400>;
+				interrupts-extended = <&exti 48 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc LPTIM2_K>;
+				clock-names = "mux";
+				wakeup-source;
+				status = "disabled";
+
+				pwm {
+					compatible = "st,stm32-pwm-lp";
+					#pwm-cells = <3>;
+					status = "disabled";
+				};
+
+				trigger@1 {
+					compatible = "st,stm32-lptimer-trigger";
+					reg = <1>;
+					status = "disabled";
+				};
+
+				counter {
+					compatible = "st,stm32-lptimer-counter";
+					status = "disabled";
+				};
+
+				timer {
+					compatible = "st,stm32-lptimer-timer";
+					status = "disabled";
+				};
+			};
+
+			lptimer3: timer@50022000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "st,stm32-lptimer";
+				reg = <0x50022000 0x400>;
+				interrupts-extended = <&exti 50 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc LPTIM3_K>;
+				clock-names = "mux";
+				wakeup-source;
+				status = "disabled";
+
+				pwm {
+					compatible = "st,stm32-pwm-lp";
+					#pwm-cells = <3>;
+					status = "disabled";
+				};
+
+				trigger@2 {
+					compatible = "st,stm32-lptimer-trigger";
+					reg = <2>;
+					status = "disabled";
+				};
+
+				timer {
+					compatible = "st,stm32-lptimer-timer";
+					status = "disabled";
+				};
+			};
+
+			hash: hash@54003000 {
+				compatible = "st,stm32mp13-hash";
+				reg = <0x54003000 0x400>;
+				interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc HASH1>;
+				resets = <&rcc HASH1_R>;
+				dmas = <&mdma 30 0x2 0x1000a02 0x0 0x0>;
+				dma-names = "in";
+				status = "disabled";
+			};
+
+			rng: rng@54004000 {
+				compatible = "st,stm32mp13-rng";
+				reg = <0x54004000 0x400>;
+				clocks = <&rcc RNG1_K>;
+				resets = <&rcc RNG1_R>;
+				status = "disabled";
+			};
+
+			fmc: memory-controller@58002000 {
+				compatible = "st,stm32mp1-fmc2-ebi";
+				reg = <0x58002000 0x1000>;
+				ranges = <0 0 0x60000000 0x04000000>, /* EBI CS 1 */
+					 <1 0 0x64000000 0x04000000>, /* EBI CS 2 */
+					 <2 0 0x68000000 0x04000000>, /* EBI CS 3 */
+					 <3 0 0x6c000000 0x04000000>, /* EBI CS 4 */
+					 <4 0 0x80000000 0x10000000>; /* NAND */
+				#address-cells = <2>;
+				#size-cells = <1>;
+				clocks = <&rcc FMC_K>;
+				resets = <&rcc FMC_R>;
+				status = "disabled";
+
+				nand-controller@4,0 {
+					compatible = "st,stm32mp1-fmc2-nfc";
+					reg = <4 0x00000000 0x1000>,
+					      <4 0x08010000 0x1000>,
+					      <4 0x08020000 0x1000>,
+					      <4 0x01000000 0x1000>,
+					      <4 0x09010000 0x1000>,
+					      <4 0x09020000 0x1000>;
+					#address-cells = <1>;
+					#size-cells = <0>;
+					interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
+					dmas = <&mdma 24 0x2 0x12000a02 0x0 0x0>,
+					       <&mdma 24 0x2 0x12000a08 0x0 0x0>,
+					       <&mdma 25 0x2 0x12000a0a 0x0 0x0>;
+					dma-names = "tx", "rx", "ecc";
+					status = "disabled";
+				};
+			};
+
+			qspi: spi@58003000 {
+				compatible = "st,stm32f469-qspi";
+				reg = <0x58003000 0x1000>, <0x70000000 0x10000000>;
+				reg-names = "qspi", "qspi_mm";
+				#address-cells = <1>;
+				#size-cells = <0>;
+				interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
+				dmas = <&mdma 26 0x2 0x10100002 0x0 0x0>,
+				       <&mdma 26 0x2 0x10100008 0x0 0x0>;
+				dma-names = "tx", "rx";
+				clocks = <&rcc QSPI_K>;
+				resets = <&rcc QSPI_R>;
+				status = "disabled";
+			};
+
+			sdmmc1: mmc@58005000 {
+				compatible = "st,stm32-sdmmc2", "arm,pl18x", "arm,primecell";
+				arm,primecell-periphid = <0x20253180>;
+				reg = <0x58005000 0x1000>, <0x58006000 0x1000>;
+				interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc SDMMC1_K>;
+				clock-names = "apb_pclk";
+				resets = <&rcc SDMMC1_R>;
+				cap-sd-highspeed;
+				cap-mmc-highspeed;
+				max-frequency = <130000000>;
+				status = "disabled";
+			};
+
+			sdmmc2: mmc@58007000 {
+				compatible = "st,stm32-sdmmc2", "arm,pl18x", "arm,primecell";
+				arm,primecell-periphid = <0x20253180>;
+				reg = <0x58007000 0x1000>, <0x58008000 0x1000>;
+				interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH>;
+				clocks = <&rcc SDMMC2_K>;
+				clock-names = "apb_pclk";
+				resets = <&rcc SDMMC2_R>;
+				cap-sd-highspeed;
+				cap-mmc-highspeed;
+				max-frequency = <130000000>;
+				status = "disabled";
+			};
+
+			usbphyc: usbphyc@5a006000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				#clock-cells = <0>;
+				compatible = "st,stm32mp1-usbphyc";
+				reg = <0x5a006000 0x1000>;
+				clocks = <&rcc USBPHY_K>;
+				resets = <&rcc USBPHY_R>;
+				vdda1v1-supply = <&scmi_reg11>;
+				vdda1v8-supply = <&scmi_reg18>;
+				status = "disabled";
+
+				usbphyc_port0: usb-phy@0 {
+					#phy-cells = <0>;
+					reg = <0>;
+				};
+
+				usbphyc_port1: usb-phy@1 {
+					#phy-cells = <1>;
+					reg = <1>;
+				};
+			};
+		};
+
 		/*
 		 * Break node order to solve dependency probe issue between
 		 * pinctrl and exti.
--- a/arch/arm/boot/dts/st/stm32mp133.dtsi
+++ b/arch/arm/boot/dts/st/stm32mp133.dtsi
@@ -33,35 +33,37 @@
 			bosch,mram-cfg = <0x1400 0 0 32 0 0 2 2>;
 			status = "disabled";
 		};
+	};
+};
+
+&etzpc {
+	adc_1: adc@48003000 {
+		compatible = "st,stm32mp13-adc-core";
+		reg = <0x48003000 0x400>;
+		interrupts = <GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH>;
+		clocks = <&rcc ADC1>, <&rcc ADC1_K>;
+		clock-names = "bus", "adc";
+		interrupt-controller;
+		#interrupt-cells = <1>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+		status = "disabled";
 
-		adc_1: adc@48003000 {
-			compatible = "st,stm32mp13-adc-core";
-			reg = <0x48003000 0x400>;
-			interrupts = <GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc ADC1>, <&rcc ADC1_K>;
-			clock-names = "bus", "adc";
-			interrupt-controller;
-			#interrupt-cells = <1>;
+		adc1: adc@0 {
+			compatible = "st,stm32mp13-adc";
+			#io-channel-cells = <1>;
 			#address-cells = <1>;
 			#size-cells = <0>;
+			reg = <0x0>;
+			interrupt-parent = <&adc_1>;
+			interrupts = <0>;
+			dmas = <&dmamux1 9 0x400 0x80000001>;
+			dma-names = "rx";
 			status = "disabled";
 
-			adc1: adc@0 {
-				compatible = "st,stm32mp13-adc";
-				#io-channel-cells = <1>;
-				#address-cells = <1>;
-				#size-cells = <0>;
-				reg = <0x0>;
-				interrupt-parent = <&adc_1>;
-				interrupts = <0>;
-				dmas = <&dmamux1 9 0x400 0x80000001>;
-				dma-names = "rx";
-				status = "disabled";
-
-				channel@18 {
-					reg = <18>;
-					label = "vrefint";
-				};
+			channel@18 {
+				reg = <18>;
+				label = "vrefint";
 			};
 		};
 	};
--- a/arch/arm/boot/dts/st/stm32mp13xc.dtsi
+++ b/arch/arm/boot/dts/st/stm32mp13xc.dtsi
@@ -4,15 +4,13 @@
  * Author: Alexandre Torgue <alexandre.torgue@foss.st.com> for STMicroelectronics.
  */
 
-/ {
-	soc {
-		cryp: crypto@54002000 {
-			compatible = "st,stm32mp1-cryp";
-			reg = <0x54002000 0x400>;
-			interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc CRYP1>;
-			resets = <&rcc CRYP1_R>;
-			status = "disabled";
-		};
+&etzpc {
+	cryp: crypto@54002000 {
+		compatible = "st,stm32mp1-cryp";
+		reg = <0x54002000 0x400>;
+		interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
+		clocks = <&rcc CRYP1>;
+		resets = <&rcc CRYP1_R>;
+		status = "disabled";
 	};
 };
--- a/arch/arm/boot/dts/st/stm32mp13xf.dtsi
+++ b/arch/arm/boot/dts/st/stm32mp13xf.dtsi
@@ -4,15 +4,13 @@
  * Author: Alexandre Torgue <alexandre.torgue@foss.st.com> for STMicroelectronics.
  */
 
-/ {
-	soc {
-		cryp: crypto@54002000 {
-			compatible = "st,stm32mp1-cryp";
-			reg = <0x54002000 0x400>;
-			interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&rcc CRYP1>;
-			resets = <&rcc CRYP1_R>;
-			status = "disabled";
-		};
+&etzpc {
+	cryp: crypto@54002000 {
+		compatible = "st,stm32mp1-cryp";
+		reg = <0x54002000 0x400>;
+		interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
+		clocks = <&rcc CRYP1>;
+		resets = <&rcc CRYP1_R>;
+		status = "disabled";
 	};
 };
