--- a/arch/arm64/boot/dts/rockchip/rk3566-nanopi-r3s.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3566-nanopi-r3s.dts
@@ -24,6 +24,11 @@
 		ethernet0 = &gmac1;
 		mmc0 = &sdhci;
 		mmc1 = &sdmmc0;
+
+		led-boot = &power_led;
+		led-failsafe = &power_led;
+		led-running = &power_led;
+		led-upgrade = &power_led;
 	};
 
 	chosen: chosen {
