From 196423a17b92ef241766691b42dac0136342bdb5 Mon Sep 17 00:00:00 2001
From: Maxim Kiselev <bigunclemax@gmail.com>
Date: Mon, 18 Dec 2023 00:06:24 +0300
Subject: [PATCH 13/14] riscv: dts: allwinner: d1: Add thermal sensor

This patch adds a thermal sensor controller node for the D1/T113s.
Also it adds a THS calibration data cell to efuse node.

Signed-off-by: Maxim Kiselev <bigunclemax@gmail.com>
Reviewed-by: Andre Przywara <andre.przywara@arm.com>
---
 .../boot/dts/allwinner/sunxi-d1s-t113.dtsi      | 17 +++++++++++++++++
 1 file changed, 17 insertions(+)

--- a/arch/riscv/boot/dts/allwinner/sunxi-d1s-t113.dtsi
+++ b/arch/riscv/boot/dts/allwinner/sunxi-d1s-t113.dtsi
@@ -166,6 +166,19 @@
 			#io-channel-cells = <1>;
 		};
 
+		ths: thermal-sensor@2009400 {
+			compatible = "allwinner,sun20i-d1-ths";
+			reg = <0x02009400 0x400>;
+			interrupts = <SOC_PERIPHERAL_IRQ(58) IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_THS>;
+			clock-names = "bus";
+			resets = <&ccu RST_BUS_THS>;
+			nvmem-cells = <&ths_calibration>;
+			nvmem-cell-names = "calibration";
+			status = "disabled";
+			#thermal-sensor-cells = <0>;
+		};
+
 		dmic: dmic@2031000 {
 			compatible = "allwinner,sun20i-d1-dmic",
 				     "allwinner,sun50i-h6-dmic";
@@ -415,6 +428,10 @@
 			reg = <0x3006000 0x1000>;
 			#address-cells = <1>;
 			#size-cells = <1>;
+
+			ths_calibration: thermal-sensor-calibration@14 {
+				reg = <0x14 0x4>;
+			};
 		};
 
 		crypto: crypto@3040000 {
