// SPDX-License-Identifier: GPL-2.0-or-later

#include "rtl8380_zyxel_gs1900.dtsi"

/ {
	compatible = "zyxel,gs1900-24ep", "realtek,rtl838x-soc";
	model = "Zyxel GS1900-24EP Switch";
};

&uart1 {
	status = "okay";
};

&mdio {
	EXTERNAL_PHY(0)
	EXTERNAL_PHY(1)
	EXTERNAL_PHY(2)
	EXTERNAL_PHY(3)
	EXTERNAL_PHY(4)
	EXTERNAL_PHY(5)
	EXTERNAL_PHY(6)
	EXTERNAL_PHY(7)

	EXTERNAL_PHY(16)
	EXTERNAL_PHY(17)
	EXTERNAL_PHY(18)
	EXTERNAL_PHY(19)
	EXTERNAL_PHY(20)
	EXTERNAL_PHY(21)
	EXTERNAL_PHY(22)
	EXTERNAL_PHY(23)
};

&switch0 {
	ports {
		SWITCH_PORT(0, 1, qsgmii)
		SWITCH_PORT(1, 2, qsgmii)
		SWITCH_PORT(2, 3, qsgmii)
		SWITCH_PORT(3, 4, qsgmii)
		SWITCH_PORT(4, 5, qsgmii)
		SWITCH_PORT(5, 6, qsgmii)
		SWITCH_PORT(6, 7, qsgmii)
		SWITCH_PORT(7, 8, qsgmii)

		SWITCH_PORT(8, 9, internal)
		SWITCH_PORT(9, 10, internal)
		SWITCH_PORT(10, 11, internal)
		SWITCH_PORT(11, 12, internal)
		SWITCH_PORT(12, 13, internal)
		SWITCH_PORT(13, 14, internal)
		SWITCH_PORT(14, 15, internal)
		SWITCH_PORT(15, 16, internal)

		SWITCH_PORT(16, 17, qsgmii)
		SWITCH_PORT(17, 18, qsgmii)
		SWITCH_PORT(18, 19, qsgmii)
		SWITCH_PORT(19, 20, qsgmii)
		SWITCH_PORT(20, 21, qsgmii)
		SWITCH_PORT(21, 22, qsgmii)
		SWITCH_PORT(22, 23, qsgmii)
		SWITCH_PORT(23, 24, qsgmii)
	};
};
