From: Joe Mullally <jwmullally@gmail.com>
Subject: mtd/spi-nor/xmc: add support for XMC XM25QH64C

The XMC XM25QH64C is a 8MB SPI NOR chip. The patch is verified on TL-WPA8631P v3.
Datasheet available at https://www.xmcwh.com/uploads/442/XM25QH64C.pdf

Signed-off-by: Joe Mullally <jwmullally@gmail.com>
---
 drivers/mtd/spi-nor/xmc.c                             | 2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/mtd/spi-nor/xmc.c
+++ b/drivers/mtd/spi-nor/xmc.c
@@ -13,6 +13,9 @@ static const struct flash_info xmc_nor_p
 	{ "XM25QH64A", INFO(0x207017, 0, 64 * 1024, 128)
 		NO_SFDP_FLAGS(SECT_4K | SPI_NOR_DUAL_READ |
 			      SPI_NOR_QUAD_READ) },
+	{ "XM25QH64C", INFO(0x204017, 0, 64 * 1024, 128)
+		NO_SFDP_FLAGS(SECT_4K | SPI_NOR_DUAL_READ |
+			      SPI_NOR_QUAD_READ) },
 	{ "XM25QH128A", INFO(0x207018, 0, 64 * 1024, 256)
 		NO_SFDP_FLAGS(SECT_4K | SPI_NOR_DUAL_READ |
 			      SPI_NOR_QUAD_READ) },
