From 9167cda9db82d0822fad0bfd609417f5fd534de8 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 23 Jun 2020 14:32:51 +0100
Subject: [PATCH 0223/1085] media: bcm2835-unicam: Add support for
 get_mbus_config to set num lanes

Use the get_mbus_config pad subdev call to allow a source to use
fewer than the number of CSI2 lanes defined in device tree.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 .../media/platform/bcm2835/bcm2835-unicam.c   | 31 ++++++++++++++++---
 1 file changed, 27 insertions(+), 4 deletions(-)

--- a/drivers/media/platform/bcm2835/bcm2835-unicam.c
+++ b/drivers/media/platform/bcm2835/bcm2835-unicam.c
@@ -1641,12 +1641,35 @@ static int unicam_start_streaming(struct
 		goto err_streaming;
 	}
 
-	/*
-	 * TODO: Retrieve the number of active data lanes from the connected
-	 * subdevice.
-	 */
 	dev->active_data_lanes = dev->max_data_lanes;
 
+	if (dev->bus_type == V4L2_MBUS_CSI2_DPHY) {
+		struct v4l2_mbus_config mbus_config = { 0 };
+
+		ret = v4l2_subdev_call(dev->sensor, pad, get_mbus_config,
+				       0, &mbus_config);
+		if (ret < 0 && ret != -ENOIOCTLCMD) {
+			unicam_dbg(3, dev, "g_mbus_config failed\n");
+			goto err_pm_put;
+		}
+
+		dev->active_data_lanes =
+			(mbus_config.flags & V4L2_MBUS_CSI2_LANE_MASK) >>
+					__ffs(V4L2_MBUS_CSI2_LANE_MASK);
+		if (!dev->active_data_lanes)
+			dev->active_data_lanes = dev->max_data_lanes;
+		if (dev->active_data_lanes > dev->max_data_lanes) {
+			unicam_err(dev, "Device has requested %u data lanes, which is >%u configured in DT\n",
+				   dev->active_data_lanes,
+				   dev->max_data_lanes);
+			ret = -EINVAL;
+			goto err_pm_put;
+		}
+	}
+
+	unicam_dbg(1, dev, "Running with %u data lanes\n",
+		   dev->active_data_lanes);
+
 	ret = clk_set_rate(dev->clock, 100 * 1000 * 1000);
 	if (ret) {
 		unicam_err(dev, "failed to set up clock\n");
