// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include <dt-bindings/leds/common.h>

#include "mt7620a_tplink_8m.dtsi"

/ {
	compatible = "tplink,archer-c2-v1", "ralink,mt7620a-soc";
	model = "TP-Link Archer C2 v1";

	aliases {
		led-boot = &led_wps;
		led-failsafe = &led_wps;
		led-running = &led_wps;
		led-upgrade = &led_wps;
	};


	leds {
		compatible = "gpio-leds";

		led-0 {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
		};

		led-1 {
			function = LED_FUNCTION_USB;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};

		led_wps: led-2 {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
		};

		led-3 {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio2 0 GPIO_ACTIVE_LOW>;
		};

		led-4 {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	rtl8367rb {
		compatible = "realtek,rtl8367b";
		realtek,extif = <6 1 0 1 1 1 1 1 1 2>;
		mii-bus = <&mdio0>;
	};
};

&state_default {
	gpio {
		groups = "i2c", "uartf", "wled", "ephy", "spi refclk";
		function = "gpio";
	};
};

&ethernet {
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii1_pins &rgmii2_pins &mdio_pins>;

	port@5 {
		status = "okay";
		mediatek,fixed-link = <1000 1 1 1>;
		phy-mode = "rgmii";
	};

	mdio0: mdio-bus {
		status = "okay";
	};
};


&wmac {
	nvmem-cells = <&eeprom_radio_0>, <&macaddr_rom_f100 0>;
	nvmem-cell-names = "eeprom", "mac-address";
};

&wifi {
	nvmem-cells = <&eeprom_radio_8000>, <&macaddr_rom_f100 (-1)>;
	nvmem-cell-names = "eeprom", "mac-address";
};
