// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "AVM FRITZ!Repeater 3000";
	compatible = "avm,fritzrepeater-3000";

	aliases {
		led-boot = &power_led;
		led-failsafe = &power_led;
		led-running = &power_led;
		led-upgrade = &power_led;
	};

	soc {
		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};

	key {
		compatible = "gpio-keys";

		connect {
			label = "Connect";
			gpios = <&tlmm 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		connect_red {
			label = "red:connect";
			gpios = <&tlmm 30 GPIO_ACTIVE_LOW>;
		};

		connect_green {
			label = "green:connect";
			gpios = <&tlmm 31 GPIO_ACTIVE_LOW>;
		};

		connect_blue {
			label = "blue:connect";
			gpios = <&tlmm 32 GPIO_ACTIVE_LOW>;
		};

		power_led: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&tlmm 33 GPIO_ACTIVE_LOW>;
		};
	};
};

&watchdog {
	status = "okay";
};

&prng {
	status = "okay";
};

&crypto {
	status = "okay";
};

&tlmm {
	serial_0_pins: serial_pinmux {
		mux {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	nand_pins: nand_pins {
		pullups {
			pins = "gpio53", "gpio58", "gpio59";
			function = "qpic";
			bias-pull-up;
		};

		pulldowns {
			pins = "gpio54", "gpio55", "gpio56",
				"gpio57", "gpio60", "gpio61",
				"gpio62", "gpio63", "gpio64",
				"gpio65", "gpio66", "gpio67",
				"gpio68", "gpio69";
			function = "qpic";
			bias-pull-down;
		};
	};
};

&nand {
	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";
	status = "okay";

	nand@0 {
		/delete-property/ nand-ecc-strength;
		/delete-property/ nand-ecc-step-size;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "SBL1";
				reg = <0x000000 0x80000>;
				read-only;
			};

			partition@80000 {
				label = "MIBIB";
				reg = <0x080000 0x80000>;
				read-only;
			};

			partition@100000 {
				label = "QSEE";
				reg = <0x100000 0x80000>;
				read-only;
			};

			partition@180000 {
				label = "CDT";
				reg = <0x180000 0x40000>;
				read-only;
			};

			partition@1c0000 {
				label = "QSEE_B";
				reg = <0x1c0000 0x80000>;
				read-only;
			};

			partition@240000 {
				label = "urlader0";
				reg = <0x240000 0x40000>;
				read-only;
			};

			partition@280000 {
				label = "urlader1";
				reg = <0x280000 0x40000>;
				read-only;
			};

			partition@2c0000 {
				label = "nand-tffs";
				reg = <0x2c0000 0x840000>;
				read-only;
			};

			partition@b00000 {
				/* 'kernel1' in AVM firmware */
				label = "uboot0";
				reg = <0xb00000 0x400000>;
			};

			partition@f00000 {
				/* 'kernel2' in AVM firmware */
				label = "uboot1";
				reg = <0xf00000 0x400000>;
			};

			partition@1300000 {
				label = "ubi";
				reg = <0x1300000 0x6d00000>;
			};
		};
	};
};

&cryptobam {
	status = "okay";
};

&blsp_dma {
	status = "okay";
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_0_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&qpic_bam {
	status = "okay";
};

&wifi0 {
	status = "okay";
	/* BDFs are identical for the FRITZ!Box 7530 and the FRITZ!Repeater 3000 */
	qcom,ath10k-calibration-variant = "AVM-FRITZRepeater-3000";
};

&wifi1 {
	status = "okay";
	ieee80211-freq-limit = <5170000 5350000>;
	/* BDFs are identical for the FRITZ!Box 7530 and the FRITZ!Repeater 3000 */
	qcom,ath10k-calibration-variant = "AVM-FRITZRepeater-3000";
};

&pcie0 {
	status = "okay";

	perst-gpio = <&tlmm 35 GPIO_ACTIVE_LOW>;
	wake-gpio = <&tlmm 50 GPIO_ACTIVE_LOW>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			/* QCA9984 */
			compatible = "qcom,ath10k";
			status = "okay";
			reg = <0x00010000 0 0 0 0>;
			ieee80211-freq-limit = <5470000 5875000>;
			/* Uses the reference BDF */
		};
	};
};

&mdio {
	status = "okay";
};

&gmac {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport4 {
	status = "okay";

	label = "lan1";
};

&swport5 {
	status = "okay";

	label = "lan2";
};
