--- /dev/null
+++ b/arch/arm/dts/mt7986a-glinet-gl-mt6000.dts
@@ -0,0 +1,135 @@
+// SPDX-License-Identifier: GPL-2.0
+
+/dts-v1/;
+#include <dt-bindings/input/linux-event-codes.h>
+#include <dt-bindings/gpio/gpio.h>
+
+#include "mt7986.dtsi"
+
+/ {
+	model = "GL.iNet GL-MT6000";
+	compatible = "glinet,gl-mt6000", "mediatek,mt7986-emmc-rfb", "mediatek,mt7986";
+
+	chosen {
+		stdout-path = &uart0;
+		tick-timer = &timer0;
+	};
+
+	memory@40000000 {
+		device_type = "memory";
+		reg = <0x40000000 0x40000000>;
+	};
+
+    reg_1p8v: regulator-1p8v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-1.8V";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+
+	reg_3p3v: regulator-3p3v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-3.3V";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+
+	keys {
+		compatible = "gpio-keys";
+
+		wps {
+			label = "reset";
+			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
+			linux,code = <KEY_RESTART>;
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		led_status_blue: green {
+			label = "blue:status";
+			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
+		};
+
+		led_status_white: blue {
+			label = "white:status";
+			gpios = <&gpio 27 GPIO_ACTIVE_LOW>;
+		};
+	};
+
+};
+
+&uart0 {
+	mediatek,force-highspeed;
+	status = "okay";
+};
+
+&eth {
+	status = "okay";
+	mediatek,gmac-id = <0>;
+	phy-mode = "2500base-x";
+	mediatek,switch = "mt7531";
+	reset-gpios = <&gpio 18 GPIO_ACTIVE_HIGH>;
+
+	fixed-link {
+		speed = <2500>;
+		full-duplex;
+	};
+};
+
+&pinctrl {
+	mmc0_pins_default: mmc0default {
+		mux {
+			function = "flash";
+			groups =  "emmc_51";
+		};
+
+		conf-cmd-dat {
+			pins = "EMMC_DATA_0", "EMMC_DATA_1", "EMMC_DATA_2",
+			       "EMMC_DATA_3", "EMMC_DATA_4", "EMMC_DATA_5",
+			       "EMMC_DATA_6", "EMMC_DATA_7", "EMMC_CMD";
+			input-enable;
+			drive-strength = <MTK_DRIVE_4mA>;
+			bias-pull-up = <MTK_PUPD_SET_R1R0_01>;
+		};
+
+		conf-clk {
+			pins = "EMMC_CK";
+			drive-strength = <MTK_DRIVE_6mA>;
+			bias-pull-down = <MTK_PUPD_SET_R1R0_10>;
+		};
+
+		conf-dsl {
+			pins = "EMMC_DSL";
+			bias-pull-down = <MTK_PUPD_SET_R1R0_10>;
+		};
+
+		conf-rst {
+			pins = "EMMC_RSTB";
+			drive-strength = <MTK_DRIVE_4mA>;
+			bias-pull-up = <MTK_PUPD_SET_R1R0_01>;
+		};
+	};
+};
+
+&mmc0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc0_pins_default>;
+	bus-width = <8>;
+	max-frequency = <200000000>;
+	cap-mmc-highspeed;
+	cap-mmc-hw-reset;
+	vmmc-supply = <&reg_3p3v>;
+	vqmmc-supply = <&reg_1p8v>;
+	non-removable;
+	status = "okay";
+};
+
+&wmcpu_emi {
+	status = "disabled";
+};
--- /dev/null
+++ b/configs/mt7986a_glinet_gl-mt6000_defconfig
@@ -0,0 +1,106 @@
+CONFIG_ARM=y
+CONFIG_SYS_HAS_NONCACHED_MEMORY=y
+CONFIG_POSITION_INDEPENDENT=y
+CONFIG_ARCH_MEDIATEK=y
+CONFIG_TEXT_BASE=0x41e00000
+CONFIG_SYS_MALLOC_F_LEN=0x4000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_ENV_SIZE=0x80000
+CONFIG_ENV_OFFSET=0x400000
+CONFIG_DEFAULT_DEVICE_TREE="mt7986a-glinet-gl-mt6000"
+CONFIG_OF_LIBFDT_OVERLAY=y
+CONFIG_TARGET_MT7986=y
+CONFIG_PRE_CON_BUF_ADDR=0x4007EF00
+CONFIG_DEBUG_UART_BASE=0x11002000
+CONFIG_DEBUG_UART_CLOCK=40000000
+CONFIG_SYS_LOAD_ADDR=0x46000000
+CONFIG_DEBUG_UART=y
+CONFIG_AHCI=y
+CONFIG_FIT=y
+CONFIG_AUTOBOOT_KEYED=y
+CONFIG_AUTOBOOT_MENU_SHOW=y
+CONFIG_DEFAULT_FDT_FILE="mediatek/mt7986a-glinet-gl-mt6000.dtb"
+CONFIG_LOGLEVEL=7
+CONFIG_PRE_CONSOLE_BUFFER=y
+CONFIG_LOG=y
+CONFIG_BOARD_LATE_INIT=y
+CONFIG_HUSH_PARSER=y
+CONFIG_SYS_PROMPT="MT7986> "
+CONFIG_CMD_CPU=y
+CONFIG_CMD_LICENSE=y
+# CONFIG_CMD_BOOTEFI_BOOTMGR is not set
+CONFIG_CMD_BOOTMENU=y
+CONFIG_CMD_ASKENV=y
+CONFIG_CMD_ERASEENV=y
+CONFIG_CMD_ENV_FLAGS=y
+CONFIG_CMD_STRINGS=y
+CONFIG_CMD_DM=y
+CONFIG_CMD_GPIO=y
+CONFIG_CMD_PWM=y
+CONFIG_CMD_GPT=y
+CONFIG_CMD_MMC=y
+CONFIG_CMD_PART=y
+CONFIG_CMD_USB=y
+CONFIG_CMD_DHCP=y
+CONFIG_CMD_TFTPSRV=y
+CONFIG_CMD_RARP=y
+CONFIG_CMD_PING=y
+CONFIG_CMD_CDP=y
+CONFIG_CMD_SNTP=y
+CONFIG_CMD_DNS=y
+CONFIG_CMD_LINK_LOCAL=y
+CONFIG_CMD_CACHE=y
+CONFIG_CMD_PSTORE=y
+CONFIG_CMD_PSTORE_MEM_ADDR=0x42ff0000
+CONFIG_CMD_UUID=y
+CONFIG_CMD_HASH=y
+CONFIG_CMD_SMC=y
+CONFIG_OF_EMBED=y
+CONFIG_ENV_OVERWRITE=y
+CONFIG_ENV_IS_IN_MMC=y
+CONFIG_SYS_RELOC_GD_ENV_ADDR=y
+CONFIG_USE_DEFAULT_ENV_FILE=y
+CONFIG_DEFAULT_ENV_FILE="glinet_gl-mt6000_env"
+CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
+CONFIG_VERSION_VARIABLE=y
+CONFIG_NET_RANDOM_ETHADDR=y
+CONFIG_NETCONSOLE=y
+CONFIG_USE_IPADDR=y
+CONFIG_IPADDR="192.168.1.1"
+CONFIG_USE_SERVERIP=y
+CONFIG_SERVERIP="192.168.1.254"
+CONFIG_REGMAP=y
+CONFIG_SYSCON=y
+CONFIG_BUTTON=y
+CONFIG_BUTTON_GPIO=y
+CONFIG_CLK=y
+CONFIG_GPIO_HOG=y
+CONFIG_LED=y
+CONFIG_LED_BLINK=y
+CONFIG_LED_GPIO=y
+CONFIG_SUPPORT_EMMC_BOOT=y
+CONFIG_MMC_HS200_SUPPORT=y
+CONFIG_MMC_MTK=y
+CONFIG_PHY_FIXED=y
+CONFIG_MEDIATEK_ETH=y
+CONFIG_PHY=y
+CONFIG_PHY_MTK_TPHY=y
+CONFIG_PINCTRL=y
+CONFIG_PINCONF=y
+CONFIG_PINCTRL_MT7986=y
+CONFIG_POWER_DOMAIN=y
+CONFIG_MTK_POWER_DOMAIN=y
+CONFIG_DM_REGULATOR=y
+CONFIG_DM_REGULATOR_FIXED=y
+CONFIG_DM_REGULATOR_GPIO=y
+CONFIG_DM_PWM=y
+CONFIG_PWM_MTK=y
+CONFIG_RAM=y
+CONFIG_DM_SERIAL=y
+CONFIG_MTK_SERIAL=y
+CONFIG_USB=y
+CONFIG_USB_XHCI_HCD=y
+CONFIG_USB_XHCI_MTK=y
+CONFIG_USB_STORAGE=y
+CONFIG_HEXDUMP=y
+CONFIG_LMB_MAX_REGIONS=64
--- /dev/null
+++ b/glinet_gl-mt6000_env
@@ -0,0 +1,25 @@
+ipaddr=192.168.1.1
+serverip=192.168.1.254
+loadaddr=0x46000000
+bootdelay=3
+bootfile_bl2=openwrt-mediatek-filogic-glinet_gl-mt6000-preloader.bin
+bootfile_fip=openwrt-mediatek-filogic-glinet_gl-mt6000-bl31-uboot.fip
+bootfile_firmware=openwrt-mediatek-filogic-glinet_gl-mt6000-squashfs-factory.bin
+bootmenu_confirm_return=askenv - Press ENTER to return to menu ; bootmenu 60
+bootmenu_title=      *** U-Boot Boot Menu for GL-iNet GL-MT6000 ***
+bootmenu_0=Startup system (Default).=run boot_system
+bootmenu_1=Load Firmware via TFTP then write to eMMC.=run boot_tftp_firmware ; run bootmenu_confirm_return
+bootmenu_2=Load BL31+U-Boot FIP via TFTP then write to eMMC.=run boot_tftp_write_fip ; run bootmenu_confirm_return
+bootmenu_3=Load BL2 preloader via TFTP then write to eMMC.=run boot_tftp_write_bl2 ; run bootmenu_confirm_return
+bootmenu_4=Reboot.=reset
+bootmenu_5=Reset all settings to factory defaults.=run reset_factory ; reset
+filesize_to_blk=setexpr cnt $filesize + 0x1ff && setexpr cnt $cnt / 0x200
+mmc_read_kernel=mmc read $loadaddr $part_addr 0x100 && imszb $loadaddr image_size && test 0x$image_size -le 0x$part_size && mmc read $loadaddr $part_addr $image_size
+boot_system=part start mmc 0 kernel part_addr && part size mmc 0 kernel part_size && run mmc_read_kernel && bootm
+boot_tftp_firmware=tftpboot $loadaddr $bootfile_firmware && run emmc_write_firmware
+boot_tftp_write_fip=tftpboot $loadaddr $bootfile_fip && run emmc_write_fip
+boot_tftp_write_bl2=tftpboot $loadaddr $bootfile_bl2 && run emmc_write_bl2
+emmc_write_firmware=part start mmc 0 kernel part_addr && run filesize_to_blk && mmc write $loadaddr $part_addr $cnt
+emmc_write_bl2=run filesize_to_blk && test 0x$cnt -le 0x800 && mmc partconf 0 1 1 1 &&  && mmc write $loadaddr 0x0 0x800 ; mmc partconf 0 1 1 0
+emmc_write_fip=part start mmc 0 fip part_addr && part size mmc 0 fip part_size && run filesize_to_blk && test 0x$cnt -le 0x$part_size && mmc write $loadaddr $part_addr $cnt
+reset_factory=eraseenv && reset
