// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "AVM FRITZ!Repeater 1200";
	compatible = "avm,fritzrepeater-1200";

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_red;
		label-mac-device = &wifi0;
	};

	soc {
		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII_RGMII5>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};

	key {
		compatible = "gpio-keys";

		wps {
			label = "WPS button";
			gpios = <&tlmm 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		power_red: power_red {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&tlmm 50 GPIO_ACTIVE_LOW>;
		};

		power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&tlmm 45 GPIO_ACTIVE_HIGH>;
		};

		power_yellow {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_YELLOW>;
			gpios = <&tlmm 49 GPIO_ACTIVE_LOW>;
		};
	};
};

&watchdog {
	status = "okay";
};

&prng {
	status = "okay";
};

&crypto {
	status = "okay";
};

&tlmm {
	serial_0_pins: serial_pinmux {
		mux {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	nand_pins: nand_pins {
		pullups {
			pins = "gpio53", "gpio58", "gpio59";
			function = "qpic";
			bias-pull-up;
		};

		pulldowns {
			pins = "gpio54", "gpio55", "gpio56",
				"gpio57", "gpio60", "gpio61",
				"gpio62", "gpio63", "gpio64",
				"gpio65", "gpio66", "gpio67",
				"gpio68", "gpio69";
			function = "qpic";
			bias-pull-down;
		};
	};

	mdio_pins: mdio_pinmux {
		mux_1 {
			pins = "gpio6";
			function = "mdio";
			bias-pull-up;
		};
		mux_2 {
			pins = "gpio7";
			function = "mdc";
			bias-pull-up;
		};
	};

	phy-reset {
		line-name = "PHY-reset";
		gpios = <19 GPIO_ACTIVE_HIGH>;
		gpio-hog;
		output-high;
	};

	phy-reset-2 {
		line-name = "PHY-reset-2";
		gpios = <47 GPIO_ACTIVE_HIGH>;
		gpio-hog;
		output-high;
	};
};

&nand {
	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";
	status = "okay";

	nand@0 {
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "SBL1";
				reg = <0x0 0x80000>;
				read-only;
			};

			partition@80000 {
				label = "MIBIB";
				reg = <0x80000 0x80000>;
				read-only;
			};

			partition@100000 {
				label = "QSEE";
				reg = <0x100000 0x80000>;
				read-only;
			};

			partition@180000 {
				label = "CDT";
				reg = <0x180000 0x40000>;
				read-only;
			};

			partition@1c0000 {
				label = "QSEE_B";
				reg = <0x1c0000 0x80000>;
				read-only;
			};

			partition@240000 {
				label = "urlader0";
				reg = <0x240000 0x40000>;
				read-only;
			};

			partition@280000 {
				label = "urlader1";
				reg = <0x280000 0x40000>;
				read-only;
			};

			partition@2c0000 {
				label = "nand-tffs";
				reg = <0x2c0000 0x840000>;
				read-only;
			};

			partition@b00000 {
				/* 'kernel1' in AVM firmware */
				label = "uboot0";
				reg = <0xb00000 0x400000>;
			};

			partition@f00000 {
				/* 'kernel2' in AVM firmware */
				label = "uboot1";
				reg = <0xf00000 0x400000>;
			};

			partition@1300000 {
				label = "ubi";
				reg = <0x1300000 0x6d00000>;
			};
		};
	};
};

&cryptobam {
	status = "okay";
};

&blsp_dma {
	status = "okay";
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_0_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&qpic_bam {
	status = "okay";
};

&wifi0 {
	status = "okay";
	qcom,ath10k-calibration-variant = "AVM-FRITZRepeater-1200";
};

&wifi1 {
	status = "okay";
	qcom,ath10k-calibration-variant = "AVM-FRITZRepeater-1200";
};

&mdio {
	status = "okay";
	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";

	ethphy: ethernet-phy@0 {
		reg = <0x0>;
	};
};

&gmac {
	status = "okay";
};

&switch {
	status = "okay";

	/delete-property/ psgmii-ethphy;
};

&swport5 {
	status = "okay";

	label = "lan";
	phy-handle = <&ethphy>;
	phy-mode = "rgmii-id";
};

&qca807x {
	status = "disabled";
};

&ethphy1 {
	status = "disabled";
};

&ethphy2 {
	status = "disabled";
};

&ethphy3 {
	status = "disabled";
};

&ethphy4 {
	status = "disabled";
};

&psgmiiphy {
	status = "disabled";
};
