// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca953x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "comfast,cf-e355ac-v2", "qca,qca9531";
	model = "COMFAST CF-E355AC V2";

	aliases {
		serial0 = &uart;
		led-boot = &led_lan;
		led-failsafe = &led_lan;
		led-upgrade = &led_lan;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		/* Single RGB led controlled via GPIO */
		compatible = "gpio-leds";

		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		led_lan: lan {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			color = <LED_COLOR_ID_BLUE>;
			function = "LED_FUNCTION_WLAN_2GHZ";
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			color = <LED_COLOR_ID_RED>;
			function = "LED_FUNCTION_WLAN_5GHZ";
			gpios = <&gpio 2 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};
	};

	watchdog {
		compatible = "linux,wdt-gpio";
		gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		hw_algo = "toggle";
		hw_margin_ms = <1200>;
		always-running;
	};
};

&eth0 {
	status = "okay";
	phy-handle = <&swphy4>;

	nvmem-cells = <&macaddr_art_0 0>;
	nvmem-cell-names = "mac-address";
};

&eth1 {
	nvmem-cells = <&macaddr_art_0 1>;
	nvmem-cell-names = "mac-address";
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&precal_art_5000>, <&macaddr_art_0 10>;
		nvmem-cell-names = "pre-calibration", "mac-address";
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "winbond,w25q128", "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x010000>;
				read-only;
			};

			partition@10000 {
				label = "art";
				reg = <0x010000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_art_0: macaddr@0 {
						compatible = "mac-base";
						reg = <0x0 0x6>;
						#nvmem-cell-cells = <1>;
					};

					cal_art_1000: calibration@1000 {
						reg = <0x1000 0x440>;
					};

					precal_art_5000: pre-calibration@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};

			partition@20000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x020000 0xfd0000>;
			};

			partition@ff0000 {
				label = "nvram";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&wdt {
	status = "disabled";
};

&wmac {
	status = "okay";

	nvmem-cells = <&cal_art_1000>, <&macaddr_art_0 2>;
	nvmem-cell-names = "calibration", "mac-address";
};
