--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -114,6 +114,18 @@ config FIREBOX_T10
 	  This board is a VPN Gateway-Router with a
 	  Freescale P1010 SoC.
 
+config MSM460
+	bool "HPE MSM460"
+	select DEFAULT_UIMAGE
+	select ARCH_REQUIRE_GPIOLIB
+	select GPIO_MPC8XXX
+	select PPC_ZIMAGE_LA3000000
+	help
+	  This option enables support for the HPE MSM460 board.
+
+	  This board is a Concurrent Dual-Band wireless access point with a
+	  Freescale P1020 SoC.
+
 config MPC8540_ADS
 	bool "Freescale MPC8540 ADS"
 	select DEFAULT_UIMAGE
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -19,6 +19,7 @@ obj8259-$(CONFIG_PPC_I8259)   += mpc85xx
 obj-$(CONFIG_MPC85xx_DS)  += mpc85xx_ds.o $(obj8259-y)
 obj-$(CONFIG_MPC85xx_MDS) += mpc85xx_mds.o
 obj-$(CONFIG_MPC85xx_RDB) += mpc85xx_rdb.o
+obj-$(CONFIG_MSM460)      += msm460.o
 obj-$(CONFIG_P1010_RDB)   += p1010rdb.o
 obj-$(CONFIG_P1022_DS)    += p1022_ds.o
 obj-$(CONFIG_P1022_RDK)   += p1022_rdk.o
