// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	aliases {
		led-boot = &led_cpu;
		led-failsafe = &led_cpu;
		led-running = &led_cpu;
		led-upgrade = &led_cpu;
		label-mac-device = &gmac0;
	};

	leds {
		compatible = "gpio-leds";

		usb {
			function = LED_FUNCTION_USB;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			trigger-sources = <&xhci_ehci_port1>;
			linux,default-trigger = "usbport";
		};

		wlan5g {
			label = "blue:wlan5g";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0radio";
		};

		wlan2g {
			label = "blue:wlan2g";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1radio";
		};

		led_cpu: cpu {
			function = LED_FUNCTION_CPU;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x20000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_uboot_1fc20: macaddr@1fc20 {
						reg = <0x1fc20 0x6>;
					};

					macaddr_uboot_1fc40: macaddr@1fc40 {
						reg = <0x1fc40 0x6>;
					};
				};
			};

			partition@20000 {
				label = "config";
				reg = <0x20000 0x10000>;
				read-only;
			};

			partition@30000 {
				label = "factory";
				reg = <0x30000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_factory_0: eeprom@0 {
						reg = <0x0 0x4da8>;
					};

					eeprom_factory_8000: eeprom@8000 {
						reg = <0x8000 0x4da8>;
					};
				};
			};

			partition@40000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x40000 0xfc0000>;
			};
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "uart3", "jtag", "wdt";
		function = "gpio";
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_uboot_1fc20>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy0>;

	nvmem-cells = <&macaddr_uboot_1fc40>;
	nvmem-cell-names = "mac-address";
};

&ethphy0 {
	/delete-property/ interrupts;
};

&switch0 {
	ports {
		port@1 {
			status = "okay";
			label = "lan1";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan3";
		};

		port@4 {
			status = "okay";
			label = "lan4";
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>;
		nvmem-cell-names = "eeprom";
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_8000>;
		nvmem-cell-names = "eeprom";
		ieee80211-freq-limit = <2400000 2500000>;
	};
};
