--- a/arch/arm64/boot/dts/mediatek/mt7622-bananapi-bpi-r64.dts
+++ b/arch/arm64/boot/dts/mediatek/mt7622-bananapi-bpi-r64.dts
@@ -21,6 +21,12 @@
 	aliases {
 		serial0 = &uart0;
 		ethernet0 = &gmac0;
+		led-boot = &led_system_green;
+		led-failsafe = &led_system_blue;
+		led-running = &led_system_green;
+		led-upgrade = &led_system_blue;
+		mmc0 = &mmc0;
+		mmc1 = &mmc1;
 	};
 
 	chosen {
@@ -44,8 +50,8 @@
 		compatible = "gpio-keys";
 
 		factory-key {
-			label = "factory";
-			linux,code = <BTN_0>;
+			label = "reset";
+			linux,code = <KEY_RESTART>;
 			gpios = <&pio 0 GPIO_ACTIVE_HIGH>;
 		};
 
@@ -59,17 +65,17 @@
 	leds {
 		compatible = "gpio-leds";
 
-		led-0 {
+		led_system_green: led-0 {
 			label = "bpi-r64:pio:green";
 			color = <LED_COLOR_ID_GREEN>;
 			gpios = <&pio 89 GPIO_ACTIVE_HIGH>;
 			default-state = "off";
 		};
 
-		led-1 {
-			label = "bpi-r64:pio:red";
-			color = <LED_COLOR_ID_RED>;
-			gpios = <&pio 88 GPIO_ACTIVE_HIGH>;
+		led_system_blue: led-1 {
+			label = "bpi-r64:pio:blue";
+			color = <LED_COLOR_ID_BLUE>;
+			gpios = <&pio 85 GPIO_ACTIVE_HIGH>;
 			default-state = "off";
 		};
 	};
