From 2b098da69f9497e725683caf67fbecf79202b7fc Mon Sep 17 00:00:00 2001
From: Hal Feng <hal.feng@starfivetech.com>
Date: Fri, 22 Mar 2024 11:33:40 +0800
Subject: [PATCH 112/116] riscv: dts: starfive: visionfive 2: Add aliases for
 i2c* and uart3

Fix the numbers of i2c and uart3.

Signed-off-by: Hal Feng <hal.feng@starfivetech.com>
---
 .../riscv/boot/dts/starfive/jh7110-starfive-visionfive-2.dtsi | 4 ++++
 1 file changed, 4 insertions(+)

--- a/arch/riscv/boot/dts/starfive/jh7110-starfive-visionfive-2.dtsi
+++ b/arch/riscv/boot/dts/starfive/jh7110-starfive-visionfive-2.dtsi
@@ -15,7 +15,10 @@
 		ethernet0 = &gmac0;
 		ethernet1 = &gmac1;
 		i2c0 = &i2c0;
+		i2c1 = &i2c1;
 		i2c2 = &i2c2;
+		i2c3 = &i2c3;
+		i2c4 = &i2c4;
 		i2c5 = &i2c5;
 		i2c6 = &i2c6;
 		mmc0 = &mmc0;
@@ -23,6 +26,7 @@
 		pcie0 = &pcie0;
 		pcie1 = &pcie1;
 		serial0 = &uart0;
+		serial3 = &uart3;
 	};
 
 	chosen {
