/* Copyright (C) 1994 Free Software Foundation, Inc.
   Contributed by Joel Sherrill (jsherril@redstone-emh2.army.mil),
     On-Line Applications Research Corporation.
 
This file is part of the GNU C Library.
 
The GNU C Library is free software; you can redistribute it and/or
modify it under the terms of the GNU Library General Public License as
published by the Free Software Foundation; either version 2 of the
License, or (at your option) any later version.
 
The GNU C Library is distributed in the hope that it will be useful,
but WITHOUT ANY WARRANTY; without even the implied warranty of
MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
Library General Public License for more details.
 
You should have received a copy of the GNU Library General Public
License along with the GNU C Library; see the file COPYING.LIB.  If
not, write to the Free Software Foundation, Inc., 675 Mass Ave,
Cambridge, MA 02139, USA.  */

/* This file contains directives for the GNU linker which are specific
to the Motorola MVME136/MVME135 boards.  */

MEMORY 
        {
        ram : org = 0x3000, l = 1M
        }

/* This value is also when the space is allocated.  If you change
this one, change the other one!!! */

heap_size = 0x20000;

SECTIONS
{
        .text 0x3000 :  
        {
          text_start = ABSOLUTE(.) ;
          *(.text)
          etext = ALIGN( 0x10 ) ;
        } 

        .data ADDR( .text ) + SIZEOF( .text ): 
        {
          data_start = . ;
          *(.data)
          edata = ALIGN( 0x10 ) ;
        }

        .bss ADDR( .data ) + SIZEOF( .data ): 
        {
          bss_start = . ;
          _bss_start = . ;
          *(.bss)
          *(COMMON)
          heap_memory = .;
          . += 0x20000;
          end = . ;
          _end = . ;
        }  
}
