From 240dad1eea22c7425197a05b8582d39adc5e548b Mon Sep 17 00:00:00 2001
From: eng33 <eng33@waveshare.com>
Date: Wed, 3 Jan 2024 11:45:04 +0800
Subject: [PATCH 0838/1085]  drivers/gpu/drm/panel:Modify the DSI mode to fix
 the problem that 7.9inch cannot be displayed

Signed-off-by: eng33 <eng33@waveshare.com>
---
 drivers/gpu/drm/panel/panel-waveshare-dsi.c | 5 ++---
 1 file changed, 2 insertions(+), 3 deletions(-)

--- a/drivers/gpu/drm/panel/panel-waveshare-dsi.c
+++ b/drivers/gpu/drm/panel/panel-waveshare-dsi.c
@@ -339,9 +339,8 @@ static int ws_panel_probe(struct i2c_cli
 	 */
 	drm_panel_add(&ts->base);
 
-	ts->dsi->mode_flags = (MIPI_DSI_MODE_VIDEO |
-			   MIPI_DSI_MODE_VIDEO_SYNC_PULSE |
-			   MIPI_DSI_MODE_LPM);
+	ts->dsi->mode_flags =  MIPI_DSI_MODE_VIDEO_HSE | MIPI_DSI_MODE_VIDEO |
+			   MIPI_DSI_CLOCK_NON_CONTINUOUS;
 	ts->dsi->format = MIPI_DSI_FMT_RGB888;
 	ts->dsi->lanes = 2;
 
