From 20e20dbe4aff72107032c4ee8e06df8488458e7a Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Fri, 23 Apr 2021 16:16:49 +0100
Subject: [PATCH 0289/1085] staging/bcm2835-isp: Fix compiler warning

The result of dividing a u32 by a size_t is an unsigned int on arm32
and a long unsigned int on arm64. Use "%zu" (the size_t format) to
remove the build warning for 64-bit builds.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 drivers/staging/vc04_services/bcm2835-isp/bcm2835-v4l2-isp.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/staging/vc04_services/bcm2835-isp/bcm2835-v4l2-isp.c
+++ b/drivers/staging/vc04_services/bcm2835-isp/bcm2835-v4l2-isp.c
@@ -1237,7 +1237,7 @@ static int bcm2835_isp_get_supported_fmt
 	if (ret) {
 		if (ret == MMAL_MSG_STATUS_ENOSPC) {
 			v4l2_err(&dev->v4l2_dev,
-				 "%s: port has more encodings than we provided space for. Some are dropped (%u vs %u).\n",
+				 "%s: port has more encodings than we provided space for. Some are dropped (%zu vs %u).\n",
 				 __func__, param_size / sizeof(u32),
 				 MAX_SUPPORTED_ENCODINGS);
 			num_encodings = MAX_SUPPORTED_ENCODINGS;
