From 71b605d32017e5b8d257db7344bc2f8e8fcc973e Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Thu, 15 Feb 2024 16:30:05 +0100
Subject: [PATCH] net: phy: aquantia: add AQR113 PHY ID

Add Aquantia AQR113 PHY ID. Aquantia AQR113 is just a chip size variant of
the already supported AQR133C where the only difference is the PHY ID
and the hw chip size.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/aquantia/aquantia_main.c | 21 +++++++++++++++++++++
 1 file changed, 21 insertions(+)

--- a/drivers/net/phy/aquantia/aquantia_main.c
+++ b/drivers/net/phy/aquantia/aquantia_main.c
@@ -26,6 +26,7 @@
 #define PHY_ID_AQR111B0	0x03a1b612
 #define PHY_ID_AQR112	0x03a1b662
 #define PHY_ID_AQR412	0x03a1b712
+#define PHY_ID_AQR113	0x31c31c40
 #define PHY_ID_AQR113C	0x31c31c12
 
 #define MDIO_PHYXS_VEND_IF_STATUS		0xe812
@@ -840,6 +841,25 @@ static struct phy_driver aqr_driver[] =
 	.link_change_notify = aqr107_link_change_notify,
 },
 {
+	PHY_ID_MATCH_MODEL(PHY_ID_AQR113),
+	.name		= "Aquantia AQR113",
+	.probe          = aqr107_probe,
+	.get_rate_matching = aqr107_get_rate_matching,
+	.config_init    = aqr107_config_init,
+	.config_aneg    = aqr_config_aneg,
+	.config_intr    = aqr_config_intr,
+	.handle_interrupt       = aqr_handle_interrupt,
+	.read_status    = aqr107_read_status,
+	.get_tunable    = aqr107_get_tunable,
+	.set_tunable    = aqr107_set_tunable,
+	.suspend        = aqr107_suspend,
+	.resume         = aqr107_resume,
+	.get_sset_count = aqr107_get_sset_count,
+	.get_strings    = aqr107_get_strings,
+	.get_stats      = aqr107_get_stats,
+	.link_change_notify = aqr107_link_change_notify,
+},
+{
 	PHY_ID_MATCH_MODEL(PHY_ID_AQR113C),
 	.name           = "Aquantia AQR113C",
 	.probe          = aqr107_probe,
@@ -874,6 +894,7 @@ static struct mdio_device_id __maybe_unu
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR111B0) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR112) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR412) },
+	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR113) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR113C) },
 	{ }
 };
