From 6fb744c8b887ffa5b0389cdae5a3e21ae0515390 Mon Sep 17 00:00:00 2001
From: Chris Morgan <macromorgan@hotmail.com>
Date: Fri, 28 Jan 2022 17:37:43 -0600
Subject: [PATCH 0340/1085] media: uapi: Document format
 MEDIA_BUS_FMT_RGB565_1X24_CPADHI

Add support for MEDIA_BUS_FMT_RGB565_1X24_CPADHI. This format is used
by the Geekworm MZP280 panel which interfaces with the Raspberry Pi.

Signed-off-by: Chris Morgan <macromorgan@hotmail.com>
---
 .../media/v4l/subdev-formats.rst              | 37 +++++++++++++++++++
 1 file changed, 37 insertions(+)

--- a/Documentation/userspace-api/media/v4l/subdev-formats.rst
+++ b/Documentation/userspace-api/media/v4l/subdev-formats.rst
@@ -624,6 +624,43 @@ The following tables list existing packe
       - b\ :sub:`2`
       - b\ :sub:`1`
       - b\ :sub:`0`
+    * .. _MEDIA_BUS_FMT_RGB565_1X24_CPADHI:
+
+      - MEDIA_BUS_FMT_RGB565_1X24_CPADHI
+      - 0x1020
+      -
+      -
+      -
+      -
+      -
+      -
+      -
+      -
+      -
+      - 0
+      - 0
+      - 0
+      - r\ :sub:`4`
+      - r\ :sub:`3`
+      - r\ :sub:`2`
+      - r\ :sub:`1`
+      - r\ :sub:`0`
+      - 0
+      - 0
+      - g\ :sub:`5`
+      - g\ :sub:`4`
+      - g\ :sub:`3`
+      - g\ :sub:`2`
+      - g\ :sub:`1`
+      - g\ :sub:`0`
+      - 0
+      - 0
+      - 0
+      - b\ :sub:`4`
+      - b\ :sub:`3`
+      - b\ :sub:`2`
+      - b\ :sub:`1`
+      - b\ :sub:`0`
     * .. _MEDIA-BUS-FMT-BGR565-2X8-BE:
 
       - MEDIA_BUS_FMT_BGR565_2X8_BE
