From 31eb43be8cad2818b4458cf1fd2dfa60031ee5f4 Mon Sep 17 00:00:00 2001
From: Matthew <sirfragles@gmail.com>
Date: Tue, 16 Jul 2024 11:20:54 +0200
Subject: [PATCH 1172/1215] Revert "Update DAC8x to support 384khz (#6187)"

This reverts commit dd7a15472b18d4bce738bb9213443c140473833b.
---
 sound/soc/bcm/rpi-simple-soundcard.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/sound/soc/bcm/rpi-simple-soundcard.c
+++ b/sound/soc/bcm/rpi-simple-soundcard.c
@@ -324,10 +324,10 @@ static int hifiberry_dac8x_init(struct s
 	struct snd_soc_dai *codec_dai = asoc_rtd_to_codec(rtd, 0);
 
 	/* override the defaults to reflect 4 x PCM5102A on the card
-	 * and limit the sample rate to 384ksps
+	 * and limit the sample rate to 192ksps
 	 */
 	codec_dai->driver->playback.channels_max = 8;
-	codec_dai->driver->playback.rates = SNDRV_PCM_RATE_8000_384000;
+	codec_dai->driver->playback.rates = SNDRV_PCM_RATE_8000_192000;
 
 	return 0;
 }
