From c927b6e47b5cc7324217bf5fe7e6ccd0633971a0 Mon Sep 17 00:00:00 2001
From: Martin Blumenstingl <martin.blumenstingl@googlemail.com>
Date: Tue, 11 Jun 2024 15:54:30 +0200
Subject: net: dsa: lantiq_gswip: Change literal 6 to ETH_ALEN

The addr variable in gswip_port_fdb_dump() stores a mac address. Use
ETH_ALEN to make this consistent across other drivers.

Signed-off-by: Martin Blumenstingl <martin.blumenstingl@googlemail.com>
Reviewed-by: Vladimir Oltean <olteanv@gmail.com>
Acked-by: Hauke Mehrtens <hauke@hauke-m.de>
Signed-off-by: Martin Schiller <ms@dev.tdt.de>
Link: https://lore.kernel.org/r/20240611135434.3180973-9-ms@dev.tdt.de
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/lantiq_gswip.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/dsa/lantiq_gswip.c
+++ b/drivers/net/dsa/lantiq_gswip.c
@@ -1406,7 +1406,7 @@ static int gswip_port_fdb_dump(struct ds
 {
 	struct gswip_priv *priv = ds->priv;
 	struct gswip_pce_table_entry mac_bridge = {0,};
-	unsigned char addr[6];
+	unsigned char addr[ETH_ALEN];
 	int i;
 	int err;
 
